From 99bed124420afaaa6aea9a80440e7fa80b27177b Mon Sep 17 00:00:00 2001
From: Jan Kiszka <jan.kiszka@siemens.com>
Date: Fri, 24 Mar 2017 18:34:16 +0100
Subject: [PATCH 19/27] efi/capsule: Clean up pr_err/info messages

Avoid __func__, improve the information provided by some of the
messages.

Signed-off-by: Jan Kiszka <jan.kiszka@siemens.com>
Reviewed-by: Matt Fleming <matt@codeblueprint.co.uk>
Signed-off-by: Ard Biesheuvel <ard.biesheuvel@linaro.org>
---
 drivers/firmware/efi/capsule-loader.c | 19 ++++++++-----------
 1 file changed, 8 insertions(+), 11 deletions(-)

diff --git a/drivers/firmware/efi/capsule-loader.c b/drivers/firmware/efi/capsule-loader.c
index 7b57dda2417d..3fb91e1597a9 100644
--- a/drivers/firmware/efi/capsule-loader.c
+++ b/drivers/firmware/efi/capsule-loader.c
@@ -70,7 +70,7 @@ static ssize_t efi_capsule_setup_info(struct capsule_info *cap_info,
 	pages_needed = ALIGN(cap_hdr->imagesize, PAGE_SIZE) >> PAGE_SHIFT;
 
 	if (pages_needed == 0) {
-		pr_err("%s: pages count invalid\n", __func__);
+		pr_err("invalid capsule size");
 		return -EINVAL;
 	}
 
@@ -79,8 +79,7 @@ static ssize_t efi_capsule_setup_info(struct capsule_info *cap_info,
 				    cap_hdr->imagesize,
 				    &cap_info->reset_type);
 	if (ret) {
-		pr_err("%s: efi_capsule_supported() failed\n",
-		       __func__);
+		pr_err("capsule not supported\n");
 		return ret;
 	}
 
@@ -115,14 +114,14 @@ static ssize_t efi_capsule_submit_update(struct capsule_info *cap_info)
 	ret = efi_capsule_update(cap_hdr_temp, cap_info->pages);
 	vunmap(cap_hdr_temp);
 	if (ret) {
-		pr_err("%s: efi_capsule_update() failed\n", __func__);
+		pr_err("capsule update failed\n");
 		return ret;
 	}
 
 	/* Indicate capsule binary uploading is done */
 	cap_info->index = NO_FURTHER_WRITE_ACTION;
-	pr_info("%s: Successfully upload capsule file with reboot type '%s'\n",
-		__func__, !cap_info->reset_type ? "RESET_COLD" :
+	pr_info("Successfully upload capsule file with reboot type '%s'\n",
+		!cap_info->reset_type ? "RESET_COLD" :
 		cap_info->reset_type == 1 ? "RESET_WARM" :
 		"RESET_SHUTDOWN");
 	return 0;
@@ -207,8 +206,7 @@ static ssize_t efi_capsule_write(struct file *file, const char __user *buff,
 	if (cap_info->header_obtained &&
 	    cap_info->count >= cap_info->total_size) {
 		if (cap_info->count > cap_info->total_size) {
-			pr_err("%s: upload size exceeded header defined size\n",
-			       __func__);
+			pr_err("capsule upload size exceeded header defined size\n");
 			ret = -EINVAL;
 			goto failed;
 		}
@@ -242,7 +240,7 @@ static int efi_capsule_flush(struct file *file, fl_owner_t id)
 	struct capsule_info *cap_info = file->private_data;
 
 	if (cap_info->index > 0) {
-		pr_err("%s: capsule upload not complete\n", __func__);
+		pr_err("capsule upload not complete\n");
 		efi_free_all_buff_pages(cap_info);
 		ret = -ECANCELED;
 	}
@@ -321,8 +319,7 @@ static int __init efi_capsule_loader_init(void)
 
 	ret = misc_register(&efi_capsule_misc);
 	if (ret)
-		pr_err("%s: Failed to register misc char file note\n",
-		       __func__);
+		pr_err("Unable to register capsule loader device\n");
 
 	return ret;
 }
-- 
2.12.0

