From 8308bdff562fc1ed24d1dc48adf984db5d8bca53 Mon Sep 17 00:00:00 2001
From: Kishon Vijay Abraham I <kishon@ti.com>
Date: Sun, 31 Oct 2021 09:02:50 +0530
Subject: [PATCH] dmaengine: ti: k3-udma: Set bchan to NULL if a channel
 request fail

bcdma_get_*() checks if bchan is already allocated by checking if it
has a NON NULL value. For the error cases, bchan will have error value
and bcdma_get_*() considers this as already allocated (PASS) since the
error values are NON NULL. This results in NULL pointer dereference
error while de-referencing bchan.

Reset the value of bchan to NULL if a channel request fails.

CC: stable@vger.kernel.org
Acked-by: Peter Ujfalusi <peter.ujfalusi@gmail.com>
Signed-off-by: Kishon Vijay Abraham I <kishon@ti.com>
---
 drivers/dma/ti/k3-udma.c | 8 ++++++--
 1 file changed, 6 insertions(+), 2 deletions(-)

diff --git a/drivers/dma/ti/k3-udma.c b/drivers/dma/ti/k3-udma.c
index 8e3fd1119a77..97228c4eb85b 100644
--- a/drivers/dma/ti/k3-udma.c
+++ b/drivers/dma/ti/k3-udma.c
@@ -1348,6 +1348,7 @@ static int bcdma_get_bchan(struct udma_chan *uc)
 {
 	struct udma_dev *ud = uc->ud;
 	enum udma_tp_level tpl;
+	int ret;
 
 	if (uc->bchan) {
 		dev_dbg(ud->dev, "chan%d: already have bchan%d allocated\n",
@@ -1365,8 +1366,11 @@ static int bcdma_get_bchan(struct udma_chan *uc)
 		tpl = ud->bchan_tpl.levels - 1;
 
 	uc->bchan = __udma_reserve_bchan(ud, tpl, -1);
-	if (IS_ERR(uc->bchan))
-		return PTR_ERR(uc->bchan);
+	if (IS_ERR(uc->bchan)) {
+		ret = PTR_ERR(uc->bchan);
+		uc->bchan = NULL;
+		return ret;
+	}
 
 	uc->tchan = uc->bchan;
 
