From 1b4bf5ef06de3e2076768afce102d1ee0196a9ee Mon Sep 17 00:00:00 2001
From: Peter Ujfalusi <peter.ujfalusi@ti.com>
Date: Tue, 8 Dec 2020 11:04:33 +0200
Subject: [PATCH] dmaengine: ti: k3-psil: Extend psil_endpoint_config for K3
 PKTDMA

commit b9366e2577a38ca5322f326cff9752c2008597c6 upstream.

Additional fields needed for K3 PKTDMA to be able to handle the mapped
channels (channels are locked to handle specific threads) and flow ranges
for these mapped threads.
PKTDMA also introduces tflow for tx channels which can not be found in
K3 UDMA architecture.

Signed-off-by: Peter Ujfalusi <peter.ujfalusi@ti.com>
Reviewed-by: Grygorii Strashko <grygorii.strashko@ti.com>
Link: https://lore.kernel.org/r/20201208090440.31792-14-peter.ujfalusi@ti.com
Signed-off-by: Vinod Koul <vkoul@kernel.org>
[s-anna@ti.com: cherry-pick commit 'b9366e2577a3' from v5.11]
Signed-off-by: Suman Anna <s-anna@ti.com>
---
 include/linux/dma/k3-psil.h | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

diff --git a/include/linux/dma/k3-psil.h b/include/linux/dma/k3-psil.h
index 1962f75fa2d3..36e22c5a0f29 100644
--- a/include/linux/dma/k3-psil.h
+++ b/include/linux/dma/k3-psil.h
@@ -50,6 +50,15 @@ enum psil_endpoint_type {
  * @channel_tpl:	Desired throughput level for the channel
  * @pdma_acc32:		ACC32 must be enabled on the PDMA side
  * @pdma_burst:		BURST must be enabled on the PDMA side
+ * @mapped_channel_id:	PKTDMA thread to channel mapping for mapped channels.
+ *			The thread must be serviced by the specified channel if
+ *			mapped_channel_id is >= 0 in case of PKTDMA
+ * @flow_start:		PKDMA flow range start of mapped channel. Unmapped
+ *			channels use flow_id == chan_id
+ * @flow_num:		PKDMA flow count of mapped channel. Unmapped channels
+ *			use flow_id == chan_id
+ * @default_flow_id:	PKDMA default (r)flow index of mapped channel.
+ *			Must be within the flow range of the mapped channel.
  */
 struct psil_endpoint_config {
 	enum psil_endpoint_type ep_type;
@@ -63,6 +72,13 @@ struct psil_endpoint_config {
 	/* PDMA properties, valid for PSIL_EP_PDMA_* */
 	unsigned pdma_acc32:1;
 	unsigned pdma_burst:1;
+
+	/* PKDMA mapped channel */
+	int mapped_channel_id;
+	/* PKTDMA tflow and rflow ranges for mapped channel */
+	u16 flow_start;
+	u16 flow_num;
+	u16 default_flow_id;
 };
 
 int psil_set_new_ep_config(struct device *dev, const char *name,
