From e61c3b62700052b819dff35f7eb2114b61a39c31 Mon Sep 17 00:00:00 2001
From: Aswath Govindraju <a-govindraju@ti.com>
Date: Sat, 29 May 2021 09:07:49 +0530
Subject: [PATCH] arm64: dts: ti: k3-am65: Add support for UHS-I modes in
 MMCSD1 subsystem

UHS-I speed modes are supported in AM65 S.R. 2.0 SoC[1].

Add support by removing the no-1-8-v tag and including the voltage
regulator device tree nodes for power cycling.

However, the 4 bit interface of AM65 SR 1.0 cannot be supported at 3.3 V or
1.8 V because of erratas i2025 and i2026 [2]. As the SD card is the primary
boot mode for development usecases, continue to enable SD card and disable
UHS-I modes in it to minimize any ageing issues happening because of
erratas.

k3-am6528-iot2050-basic and k3-am6548-iot2050-advanced boards use S.R. 1.0
version of AM65 SoC. Therefore, add no-1-8-v in sdhci1 device tree node of
the common iot2050 device tree file.

[1] - https://www.ti.com/lit/ug/spruid7e/spruid7e.pdf, section 12.3.6.1.1
[2] - https://www.ti.com/lit/er/sprz452e/sprz452e.pdf

Signed-off-by: Aswath Govindraju <a-govindraju@ti.com>
Acked-by: Jan Kiszka <jan.kiszka@siemens.com>
Signed-off-by: Nishanth Menon <nm@ti.com>
Link: https://lore.kernel.org/r/20210529033749.6250-1-a-govindraju@ti.com
---
 .../boot/dts/ti/k3-am65-iot2050-common.dtsi   |  1 +
 arch/arm64/boot/dts/ti/k3-am65-main.dtsi      |  1 -
 .../arm64/boot/dts/ti/k3-am654-base-board.dts | 33 +++++++++++++++++++
 3 files changed, 34 insertions(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/ti/k3-am65-iot2050-common.dtsi b/arch/arm64/boot/dts/ti/k3-am65-iot2050-common.dtsi
index f4ec9ed52939..d90abda1de84 100644
--- a/arch/arm64/boot/dts/ti/k3-am65-iot2050-common.dtsi
+++ b/arch/arm64/boot/dts/ti/k3-am65-iot2050-common.dtsi
@@ -555,6 +555,7 @@ &sdhci1 {
 	pinctrl-0 = <&main_mmc1_pins_default>;
 	ti,driver-strength-ohm = <50>;
 	disable-wp;
+	no-1-8-v;
 };
 
 &usb0 {
diff --git a/arch/arm64/boot/dts/ti/k3-am65-main.dtsi b/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
index 75afafdcee6f..c288d03da908 100644
--- a/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
+++ b/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
@@ -304,7 +304,6 @@ sdhci1: mmc@4fa0000 {
 		ti,otap-del-sel = <0x2>;
 		ti,trm-icp = <0x8>;
 		dma-coherent;
-		no-1-8-v;
 	};
 
 	scm_conf: scm-conf@100000 {
diff --git a/arch/arm64/boot/dts/ti/k3-am654-base-board.dts b/arch/arm64/boot/dts/ti/k3-am654-base-board.dts
index 8c082af489f5..fea6a8243d75 100644
--- a/arch/arm64/boot/dts/ti/k3-am654-base-board.dts
+++ b/arch/arm64/boot/dts/ti/k3-am654-base-board.dts
@@ -60,6 +60,38 @@ clk_ov5640_fixed: clock {
 		#clock-cells = <0>;
 		clock-frequency = <24000000>;
 	};
+
+	evm_12v0: fixedregulator-evm12v0 {
+		/* main supply */
+		compatible = "regulator-fixed";
+		regulator-name = "evm_12v0";
+		regulator-min-microvolt = <12000000>;
+		regulator-max-microvolt = <12000000>;
+		regulator-always-on;
+		regulator-boot-on;
+	};
+
+	vcc3v3_io: fixedregulator-vcc3v3io {
+		/* Output of TPS54334 */
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_io";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-always-on;
+		regulator-boot-on;
+		vin-supply = <&evm_12v0>;
+	};
+
+	vdd_mmc1_sd: fixedregulator-sd {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd_mmc1_sd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		enable-active-high;
+		vin-supply = <&vcc3v3_io>;
+		gpio = <&pca9554 4 GPIO_ACTIVE_HIGH>;
+	};
 };
 
 &wkup_pmx0 {
@@ -319,6 +351,7 @@ &sdhci0 {
  * disable sdhci1
  */
 &sdhci1 {
+	vmmc-supply = <&vdd_mmc1_sd>;
 	pinctrl-names = "default";
 	pinctrl-0 = <&main_mmc1_pins_default>;
 	ti,driver-strength-ohm = <50>;
