From 3f592d3a8794d4db3192b71a7f8df363cb1c2c62 Mon Sep 17 00:00:00 2001
From: Peter Ujfalusi <peter.ujfalusi@ti.com>
Date: Tue, 8 Dec 2020 11:04:24 +0200
Subject: [PATCH] dmaengine: ti: k3-udma-glue: Add function to get device
 pointer for DMA API

Glue layer users should use the device of the DMA for DMA mapping and
allocations as it is the DMA which accesses to descriptors and buffers,
not the clients

Signed-off-by: Peter Ujfalusi <peter.ujfalusi@ti.com>
Reviewed-by: Grygorii Strashko <grygorii.strashko@ti.com>
Link: https://lore.kernel.org/r/20201208090440.31792-5-peter.ujfalusi@ti.com
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/dma/ti/k3-udma-glue.c    | 14 ++++++++++++++
 drivers/dma/ti/k3-udma-private.c |  6 ++++++
 drivers/dma/ti/k3-udma.h         |  1 +
 include/linux/dma/k3-udma-glue.h |  4 ++++
 4 files changed, 25 insertions(+)

diff --git a/drivers/dma/ti/k3-udma-glue.c b/drivers/dma/ti/k3-udma-glue.c
index a367584f0d7b..a53bc4707ae8 100644
--- a/drivers/dma/ti/k3-udma-glue.c
+++ b/drivers/dma/ti/k3-udma-glue.c
@@ -487,6 +487,13 @@ int k3_udma_glue_tx_get_irq(struct k3_udma_glue_tx_channel *tx_chn)
 }
 EXPORT_SYMBOL_GPL(k3_udma_glue_tx_get_irq);
 
+struct device *
+	k3_udma_glue_tx_get_dma_device(struct k3_udma_glue_tx_channel *tx_chn)
+{
+	return xudma_get_device(tx_chn->common.udmax);
+}
+EXPORT_SYMBOL_GPL(k3_udma_glue_tx_get_dma_device);
+
 static int k3_udma_glue_cfg_rx_chn(struct k3_udma_glue_rx_channel *rx_chn)
 {
 	const struct udma_tisci_rm *tisci_rm = rx_chn->common.tisci_rm;
@@ -1189,3 +1196,10 @@ int k3_udma_glue_rx_get_irq(struct k3_udma_glue_rx_channel *rx_chn,
 	return flow->virq;
 }
 EXPORT_SYMBOL_GPL(k3_udma_glue_rx_get_irq);
+
+struct device *
+	k3_udma_glue_rx_get_dma_device(struct k3_udma_glue_rx_channel *rx_chn)
+{
+	return xudma_get_device(rx_chn->common.udmax);
+}
+EXPORT_SYMBOL_GPL(k3_udma_glue_rx_get_dma_device);
diff --git a/drivers/dma/ti/k3-udma-private.c b/drivers/dma/ti/k3-udma-private.c
index dadab2feca08..bae6150b1d8d 100644
--- a/drivers/dma/ti/k3-udma-private.c
+++ b/drivers/dma/ti/k3-udma-private.c
@@ -50,6 +50,12 @@ struct udma_dev *of_xudma_dev_get(struct device_node *np, const char *property)
 }
 EXPORT_SYMBOL(of_xudma_dev_get);
 
+struct device *xudma_get_device(struct udma_dev *ud)
+{
+	return ud->dev;
+}
+EXPORT_SYMBOL(xudma_get_device);
+
 u32 xudma_dev_get_psil_base(struct udma_dev *ud)
 {
 	return ud->psil_base;
diff --git a/drivers/dma/ti/k3-udma.h b/drivers/dma/ti/k3-udma.h
index 09c4529e013d..d1cace0cb43b 100644
--- a/drivers/dma/ti/k3-udma.h
+++ b/drivers/dma/ti/k3-udma.h
@@ -112,6 +112,7 @@ int xudma_navss_psil_unpair(struct udma_dev *ud, u32 src_thread,
 			    u32 dst_thread);
 
 struct udma_dev *of_xudma_dev_get(struct device_node *np, const char *property);
+struct device *xudma_get_device(struct udma_dev *ud);
 void xudma_dev_put(struct udma_dev *ud);
 u32 xudma_dev_get_psil_base(struct udma_dev *ud);
 struct udma_tisci_rm *xudma_dev_get_tisci_rm(struct udma_dev *ud);
diff --git a/include/linux/dma/k3-udma-glue.h b/include/linux/dma/k3-udma-glue.h
index 5eb34ad973a7..d7c12f31377c 100644
--- a/include/linux/dma/k3-udma-glue.h
+++ b/include/linux/dma/k3-udma-glue.h
@@ -41,6 +41,8 @@ void k3_udma_glue_reset_tx_chn(struct k3_udma_glue_tx_channel *tx_chn,
 u32 k3_udma_glue_tx_get_hdesc_size(struct k3_udma_glue_tx_channel *tx_chn);
 u32 k3_udma_glue_tx_get_txcq_id(struct k3_udma_glue_tx_channel *tx_chn);
 int k3_udma_glue_tx_get_irq(struct k3_udma_glue_tx_channel *tx_chn);
+struct device *
+	k3_udma_glue_tx_get_dma_device(struct k3_udma_glue_tx_channel *tx_chn);
 
 enum {
 	K3_UDMA_GLUE_SRC_TAG_LO_KEEP = 0,
@@ -130,5 +132,7 @@ int k3_udma_glue_rx_flow_enable(struct k3_udma_glue_rx_channel *rx_chn,
 				u32 flow_idx);
 int k3_udma_glue_rx_flow_disable(struct k3_udma_glue_rx_channel *rx_chn,
 				 u32 flow_idx);
+struct device *
+	k3_udma_glue_rx_get_dma_device(struct k3_udma_glue_rx_channel *rx_chn);
 
 #endif /* K3_UDMA_GLUE_H_ */
