From 74a16f0f4302803e576a23e5d6d32b889e2cbb24 Mon Sep 17 00:00:00 2001
From: Peter Ujfalusi <peter.ujfalusi@ti.com>
Date: Sun, 25 Oct 2020 12:10:04 -0700
Subject: [PATCH] soc: ti: ti_sci_inta_msi: Add support for second range in
 resource ranges

Allocate MSI entries for both first and second range if they are valid

Signed-off-by: Peter Ujfalusi <peter.ujfalusi@ti.com>
Signed-off-by: Santosh Shilimkar <santosh.shilimkar@oracle.com>
---
 drivers/soc/ti/ti_sci_inta_msi.c | 12 ++++++++++++
 1 file changed, 12 insertions(+)

diff --git a/drivers/soc/ti/ti_sci_inta_msi.c b/drivers/soc/ti/ti_sci_inta_msi.c
index 0eb9462f609e..a1d9c027022a 100644
--- a/drivers/soc/ti/ti_sci_inta_msi.c
+++ b/drivers/soc/ti/ti_sci_inta_msi.c
@@ -89,6 +89,18 @@ static int ti_sci_inta_msi_alloc_descs(struct device *dev,
 			list_add_tail(&msi_desc->list, dev_to_msi_list(dev));
 			count++;
 		}
+		for (i = 0; i < res->desc[set].num_sec; i++) {
+			msi_desc = alloc_msi_entry(dev, 1, NULL);
+			if (!msi_desc) {
+				ti_sci_inta_msi_free_descs(dev);
+				return -ENOMEM;
+			}
+
+			msi_desc->inta.dev_index = res->desc[set].start_sec + i;
+			INIT_LIST_HEAD(&msi_desc->list);
+			list_add_tail(&msi_desc->list, dev_to_msi_list(dev));
+			count++;
+		}
 	}
 
 	return count;
