From 6f17bb476e05d69a1d950494c1b3e6db7342dc24 Mon Sep 17 00:00:00 2001
From: Jan Kiszka <jan.kiszka@siemens.com>
Date: Wed, 2 Jun 2021 08:56:15 +0200
Subject: [PATCH] arm64: dts: ti: iot2050: Configure r5f cluster on basic
 variant in split mode

Lockstep mode is not supported here. So turn it off to avoid warnings
during startup.

Signed-off-by: Jan Kiszka <jan.kiszka@siemens.com>
Signed-off-by: Nishanth Menon <nm@ti.com>
Link: https://lore.kernel.org/r/3a241e50-80a3-992a-2445-345c629d7895@siemens.com
---
 arch/arm64/boot/dts/ti/k3-am6528-iot2050-basic.dts | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm64/boot/dts/ti/k3-am6528-iot2050-basic.dts b/arch/arm64/boot/dts/ti/k3-am6528-iot2050-basic.dts
index 4f7e3f2a6265..94bb5dd39122 100644
--- a/arch/arm64/boot/dts/ti/k3-am6528-iot2050-basic.dts
+++ b/arch/arm64/boot/dts/ti/k3-am6528-iot2050-basic.dts
@@ -59,3 +59,8 @@ &main_uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&main_uart0_pins_default>;
 };
+
+&mcu_r5fss0 {
+	/* lock-step mode not supported on this board */
+	ti,cluster-mode = <0>;
+};
