From 7288ba471be4e1025c286d5673b3a177409316a0 Mon Sep 17 00:00:00 2001
From: Peter Ujfalusi <peter.ujfalusi@ti.com>
Date: Sun, 25 Oct 2020 12:10:02 -0700
Subject: [PATCH] firmware: ti_sci: rm: Add support for tx_tdtype parameter for
 tx channel

The system controller's resource manager have support for configuring the
TDTYPE of TCHAN_CFG register on j721e.
With this parameter the teardown completion can be controlled:
TDTYPE == 0: Return without waiting for peer to complete the teardown
TDTYPE == 1: Wait for peer to complete the teardown

Signed-off-by: Peter Ujfalusi <peter.ujfalusi@ti.com>
Reviewed-by: Tero Kristo <t-kristo@ti.com>
Tested-by: Keerthy <j-keerthy@ti.com>
Reviewed-by: Grygorii Strashko <grygorii.strashko@ti.com>
Signed-off-by: Santosh Shilimkar <santosh.shilimkar@oracle.com>
---
 drivers/firmware/ti_sci.c              | 1 +
 drivers/firmware/ti_sci.h              | 7 +++++++
 include/linux/soc/ti/ti_sci_protocol.h | 2 ++
 3 files changed, 10 insertions(+)

diff --git a/drivers/firmware/ti_sci.c b/drivers/firmware/ti_sci.c
index 896f53ec7857..65a8c2e82093 100644
--- a/drivers/firmware/ti_sci.c
+++ b/drivers/firmware/ti_sci.c
@@ -2362,6 +2362,7 @@ static int ti_sci_cmd_rm_udmap_tx_ch_cfg(const struct ti_sci_handle *handle,
 	req->fdepth = params->fdepth;
 	req->tx_sched_priority = params->tx_sched_priority;
 	req->tx_burst_size = params->tx_burst_size;
+	req->tx_tdtype = params->tx_tdtype;
 
 	ret = ti_sci_do_xfer(info, xfer);
 	if (ret) {
diff --git a/drivers/firmware/ti_sci.h b/drivers/firmware/ti_sci.h
index 57cd04062994..dca19ca5fc49 100644
--- a/drivers/firmware/ti_sci.h
+++ b/drivers/firmware/ti_sci.h
@@ -910,6 +910,7 @@ struct rm_ti_sci_msg_udmap_rx_flow_opt_cfg {
  *   12 - Valid bit for @ref ti_sci_msg_rm_udmap_tx_ch_cfg::tx_credit_count
  *   13 - Valid bit for @ref ti_sci_msg_rm_udmap_tx_ch_cfg::fdepth
  *   14 - Valid bit for @ref ti_sci_msg_rm_udmap_tx_ch_cfg::tx_burst_size
+ *   15 - Valid bit for @ref ti_sci_msg_rm_udmap_tx_ch_cfg::tx_tdtype
  *
  * @nav_id: SoC device ID of Navigator Subsystem where tx channel is located
  *
@@ -973,6 +974,11 @@ struct rm_ti_sci_msg_udmap_rx_flow_opt_cfg {
  *
  * @tx_burst_size: UDMAP transmit channel burst size configuration to be
  * programmed into the tx_burst_size field of the TCHAN_TCFG register.
+ *
+ * @tx_tdtype: UDMAP transmit channel teardown type configuration to be
+ * programmed into the tdtype field of the TCHAN_TCFG register:
+ * 0 - Return immediately
+ * 1 - Wait for completion message from remote peer
  */
 struct ti_sci_msg_rm_udmap_tx_ch_cfg_req {
 	struct ti_sci_msg_hdr hdr;
@@ -994,6 +1000,7 @@ struct ti_sci_msg_rm_udmap_tx_ch_cfg_req {
 	u16 fdepth;
 	u8 tx_sched_priority;
 	u8 tx_burst_size;
+	u8 tx_tdtype;
 } __packed;
 
 /**
diff --git a/include/linux/soc/ti/ti_sci_protocol.h b/include/linux/soc/ti/ti_sci_protocol.h
index b1af87330f86..fece890e1635 100644
--- a/include/linux/soc/ti/ti_sci_protocol.h
+++ b/include/linux/soc/ti/ti_sci_protocol.h
@@ -345,6 +345,7 @@ struct ti_sci_msg_rm_udmap_tx_ch_cfg {
 #define TI_SCI_MSG_VALUE_RM_UDMAP_CH_TX_SUPR_TDPKT_VALID        BIT(11)
 #define TI_SCI_MSG_VALUE_RM_UDMAP_CH_TX_CREDIT_COUNT_VALID      BIT(12)
 #define TI_SCI_MSG_VALUE_RM_UDMAP_CH_TX_FDEPTH_VALID            BIT(13)
+#define TI_SCI_MSG_VALUE_RM_UDMAP_CH_TX_TDTYPE_VALID            BIT(15)
 	u16 nav_id;
 	u16 index;
 	u8 tx_pause_on_err;
@@ -362,6 +363,7 @@ struct ti_sci_msg_rm_udmap_tx_ch_cfg {
 	u16 fdepth;
 	u8 tx_sched_priority;
 	u8 tx_burst_size;
+	u8 tx_tdtype;
 };
 
 /**
