From 187ddbf1c2b3ad2e0c4dd755fe1e240a4c85564c Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Fri, 13 Nov 2020 15:18:24 -0600
Subject: [PATCH] arm64: dts: ti: am65/j721e: Fix up un-necessary status set to
 "okay" for crypto

The default state of a device tree node is "okay". There is no specific
use of explicitly adding status = "okay" in the SoC dtsi.

Signed-off-by: Nishanth Menon <nm@ti.com>
Reviewed-by: Tony Lindgren <tony@atomide.com>
Reviewed-by: Keerthy <j-keerthy@ti.com>
Acked-by: Tero Kristo <t-kristo@ti.com>
Cc: Keerthy <j-keerthy@ti.com>
Link: https://lore.kernel.org/r/20201113211826.13087-4-nm@ti.com
---
 arch/arm64/boot/dts/ti/k3-am65-main.dtsi  | 1 -
 arch/arm64/boot/dts/ti/k3-j721e-main.dtsi | 2 --
 2 files changed, 3 deletions(-)

diff --git a/arch/arm64/boot/dts/ti/k3-am65-main.dtsi b/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
index ee7b7c356f01..ba1529436128 100644
--- a/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
+++ b/arch/arm64/boot/dts/ti/k3-am65-main.dtsi
@@ -122,7 +122,6 @@ crypto: crypto@4e00000 {
 		#address-cells = <2>;
 		#size-cells = <2>;
 		ranges = <0x0 0x04e00000 0x00 0x04e00000 0x0 0x30000>;
-		status = "okay";
 
 		dmas = <&main_udmap 0xc000>, <&main_udmap 0x4000>,
 				<&main_udmap 0x4001>;
diff --git a/arch/arm64/boot/dts/ti/k3-j721e-main.dtsi b/arch/arm64/boot/dts/ti/k3-j721e-main.dtsi
index 0350ddfe2c72..b8ca6e03de36 100644
--- a/arch/arm64/boot/dts/ti/k3-j721e-main.dtsi
+++ b/arch/arm64/boot/dts/ti/k3-j721e-main.dtsi
@@ -362,8 +362,6 @@ main_crypto: crypto@4e00000 {
 		#size-cells = <2>;
 		ranges = <0x0 0x04e00000 0x00 0x04e00000 0x0 0x30000>;
 
-		status = "okay";
-
 		dmas = <&main_udmap 0xc000>, <&main_udmap 0x4000>,
 				<&main_udmap 0x4001>;
 		dma-names = "tx", "rx1", "rx2";
