auto lo
auto eth0
auto eth1

iface lo inet loopback

iface eth0 inet dhcp

iface eth1 inet static
       address 192.168.100.200
       netmask 255.255.255.0
       broadcast 192.168.100.255


##iface wlan0 inet dhcp
##	wpa-conf /etc/wpa_supplicant/wpa_supplicant.conf

iface wlan0 inet static
	post-up hostapd -B /etc/hostapd/hostapd.conf
	post-up echo 1 > /sys/class/leds/user-led1-green/brightness
	address 192.168.10.200
	netmask 255.255.255.0
	broadcast 192.168.10.255
	down echo 0 > /sys/class/leds/user-led1-green/brightness
	down killall hostapd
	down ip addr flush dev wlan0
