auto lo
auto eth0
auto eth1
auto usb0

iface lo inet loopback

iface eth0 inet dhcp

#iface eth0 inet static
#       address 192.168.21.84
#       netmask 255.255.252.0
#       broadcast 192.168.23.255
#       gateway 192.168.21.111
#       post-up echo "nameserver 192.168.21.111" > /etc/resolv.conf

iface eth1 inet static
       address 192.168.0.1
       netmask 255.255.255.0
       broadcast 192.168.0.255

iface usb0 inet static
	address 192.168.7.2
	broadcast 192.168.7.2
	netmask 255.255.255.252

