From 05fa83d5672bc9469f05f678ddca541982d202d7 Mon Sep 17 00:00:00 2001
From: Arnd Bergmann <arnd@arndb.de>
Date: Mon, 26 Oct 2020 17:05:23 +0100
Subject: [PATCH] remoteproc: ti_k3: fix -Wcast-function-type warning

The function cast causes a warning with "make W=1"

drivers/remoteproc/ti_k3_r5_remoteproc.c: In function 'k3_r5_probe':
drivers/remoteproc/ti_k3_r5_remoteproc.c:1368:12: warning: cast between incompatible function types from 'int (*)(struct platform_device *)' to 'void (*)(void *)' [-Wcast-function-type]

Rewrite the code to avoid the cast, and fix the incorrect return
type of the callback.

Fixes: 6dedbd1d5443 ("remoteproc: k3-r5: Add a remoteproc driver for R5F subsystem")
Signed-off-by: Arnd Bergmann <arnd@arndb.de>
Link: https://lore.kernel.org/r/20201026160533.3705998-1-arnd@kernel.org
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
---
 drivers/remoteproc/ti_k3_r5_remoteproc.c | 18 ++++++------------
 1 file changed, 6 insertions(+), 12 deletions(-)

diff --git a/drivers/remoteproc/ti_k3_r5_remoteproc.c b/drivers/remoteproc/ti_k3_r5_remoteproc.c
index f92a18c06d80..e5346251db0f 100644
--- a/drivers/remoteproc/ti_k3_r5_remoteproc.c
+++ b/drivers/remoteproc/ti_k3_r5_remoteproc.c
@@ -940,9 +940,9 @@ static int k3_r5_cluster_rproc_init(struct platform_device *pdev)
 	return ret;
 }
 
-static int k3_r5_cluster_rproc_exit(struct platform_device *pdev)
+static void k3_r5_cluster_rproc_exit(void *data)
 {
-	struct k3_r5_cluster *cluster = platform_get_drvdata(pdev);
+	struct k3_r5_cluster *cluster = platform_get_drvdata(data);
 	struct k3_r5_rproc *kproc;
 	struct k3_r5_core *core;
 	struct rproc *rproc;
@@ -967,8 +967,6 @@ static int k3_r5_cluster_rproc_exit(struct platform_device *pdev)
 		rproc_free(rproc);
 		core->rproc = NULL;
 	}
-
-	return 0;
 }
 
 static int k3_r5_core_of_get_internal_memories(struct platform_device *pdev,
@@ -1255,9 +1253,9 @@ static void k3_r5_core_of_exit(struct platform_device *pdev)
 	devres_release_group(dev, k3_r5_core_of_init);
 }
 
-static void k3_r5_cluster_of_exit(struct platform_device *pdev)
+static void k3_r5_cluster_of_exit(void *data)
 {
-	struct k3_r5_cluster *cluster = platform_get_drvdata(pdev);
+	struct k3_r5_cluster *cluster = platform_get_drvdata(data);
 	struct platform_device *cpdev;
 	struct k3_r5_core *core, *temp;
 
@@ -1353,9 +1351,7 @@ static int k3_r5_probe(struct platform_device *pdev)
 		return ret;
 	}
 
-	ret = devm_add_action_or_reset(dev,
-				       (void(*)(void *))k3_r5_cluster_of_exit,
-				       pdev);
+	ret = devm_add_action_or_reset(dev, k3_r5_cluster_of_exit, pdev);
 	if (ret)
 		return ret;
 
@@ -1366,9 +1362,7 @@ static int k3_r5_probe(struct platform_device *pdev)
 		return ret;
 	}
 
-	ret = devm_add_action_or_reset(dev,
-				       (void(*)(void *))k3_r5_cluster_rproc_exit,
-				       pdev);
+	ret = devm_add_action_or_reset(dev, k3_r5_cluster_rproc_exit, pdev);
 	if (ret)
 		return ret;
 
