From c5994894f089bf55ff5cda47d29b69a7bd03cd13 Mon Sep 17 00:00:00 2001
From: Kishon Vijay Abraham I <kishon@ti.com>
Date: Wed, 10 Nov 2021 13:13:43 +0530
Subject: [PATCH] PCI: keystone: Add quirk to mark AM654 RC BAR flag as
 IORESOURCE_UNSET

AM654 RootComplex has a hard coded 64 bit BAR of size 1MB and also has
both MSI and MSI-X capability in it's config space. If PCIEPORTBUS is
enabled, it tries to configure MSI-X and msix_mask_all() adds about 10
Second boot up delay when it tries to write to undefined location.

Add quirk to mark AM654 RC BAR flag as IORESOURCE_UNSET so that
msix_map_region() returns NULL for Root Complex and avoid un-desirable
writes to MSI-X table.

Signed-off-by: Kishon Vijay Abraham I <kishon@ti.com>
Signed-off-by: Vignesh Raghavendra <vigneshr@ti.com>
---
 drivers/pci/controller/dwc/pci-keystone.c | 8 +++++++-
 1 file changed, 7 insertions(+), 1 deletion(-)

diff --git a/drivers/pci/controller/dwc/pci-keystone.c b/drivers/pci/controller/dwc/pci-keystone.c
index bb7190400ba8..4e973f829436 100644
--- a/drivers/pci/controller/dwc/pci-keystone.c
+++ b/drivers/pci/controller/dwc/pci-keystone.c
@@ -650,8 +650,14 @@ static void ks_pcie_quirk(struct pci_dev *dev)
 		{ 0, },
 	};
 
-	if (pci_is_root_bus(bus))
+	if (pci_is_root_bus(bus)) {
 		bridge = dev;
+		if (pci_match_id(am6_pci_devids, bridge)) {
+			struct resource *r = &dev->resource[0];
+
+			r->flags |= IORESOURCE_UNSET;
+		}
+	}
 
 	/* look for the host bridge */
 	while (!pci_is_root_bus(bus)) {
