From c825c3a811080c0f36390ff48910e4b9f5d5e527 Mon Sep 17 00:00:00 2001
From: Suman Anna <s-anna@ti.com>
Date: Wed, 7 Apr 2021 10:56:39 -0500
Subject: [PATCH] remoteproc: pru: Fixup interrupt-parent logic for fw events

The PRU firmware interrupt mapping logic in pru_handle_intrmap() uses
of_irq_find_parent() with PRU device node to get a handle to the PRUSS
Interrupt Controller at present. This logic however requires that the
PRU nodes always define a interrupt-parent property. This property is
neither a required/defined property as per the PRU remoteproc binding,
nor is relevant from a DT node point of view without any associated
interrupts. The current logic finds a wrong interrupt controller and
fails to perform proper mapping without any interrupt-parent property
in the PRU nodes.

Fix this logic to always find and use the sibling interrupt controller.
Also, while at this, fix the acquired interrupt controller device node
reference properly.

Fixes: c75c9fdac66e ("remoteproc: pru: Add support for PRU specific interrupt configuration")
Signed-off-by: Suman Anna <s-anna@ti.com>
Reviewed-by: Mathieu Poirier <mathieu.poirier@linaro.org>
Link: https://lore.kernel.org/r/20210407155641.5501-2-s-anna@ti.com
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
---
 drivers/remoteproc/pru_rproc.c | 15 ++++++++++++---
 1 file changed, 12 insertions(+), 3 deletions(-)

diff --git a/drivers/remoteproc/pru_rproc.c b/drivers/remoteproc/pru_rproc.c
index 21105592a83d..773c09d01958 100644
--- a/drivers/remoteproc/pru_rproc.c
+++ b/drivers/remoteproc/pru_rproc.c
@@ -284,7 +284,7 @@ static int pru_handle_intrmap(struct rproc *rproc)
 	struct pru_rproc *pru = rproc->priv;
 	struct pru_irq_rsc *rsc = pru->pru_interrupt_map;
 	struct irq_fwspec fwspec;
-	struct device_node *irq_parent;
+	struct device_node *parent, *irq_parent;
 	int i, ret = 0;
 
 	/* not having pru_interrupt_map is not an error */
@@ -312,9 +312,16 @@ static int pru_handle_intrmap(struct rproc *rproc)
 
 	/*
 	 * parse and fill in system event to interrupt channel and
-	 * channel-to-host mapping
+	 * channel-to-host mapping. The interrupt controller to be used
+	 * for these mappings for a given PRU remoteproc is always its
+	 * corresponding sibling PRUSS INTC node.
 	 */
-	irq_parent = of_irq_find_parent(pru->dev->of_node);
+	parent = of_get_parent(dev_of_node(pru->dev));
+	if (!parent)
+		return -ENODEV;
+
+	irq_parent = of_get_child_by_name(parent, "interrupt-controller");
+	of_node_put(parent);
 	if (!irq_parent) {
 		kfree(pru->mapped_irq);
 		return -ENODEV;
@@ -337,11 +344,13 @@ static int pru_handle_intrmap(struct rproc *rproc)
 			goto map_fail;
 		}
 	}
+	of_node_put(irq_parent);
 
 	return ret;
 
 map_fail:
 	pru_dispose_irq_mapping(pru);
+	of_node_put(irq_parent);
 
 	return ret;
 }
